**SBL Series Indoor Blank-out LED Backlit Sign**

The SBL Series Indoor, Blank-out, LED Backlit sign is designed with a matrix of energy efficient LEDs illuminating a block-style message. The sign features blank-out technology that only displays the sign message when illuminated.

It is engineered with a solid-state circuit board and switch-mode power supply for maximum LED life. The cabinet is constructed of corrosion-resistant, extruded aluminum and ships with our built-in Lift'N Shift back for wall mounting. Ceiling, post, wall-projection and recessed mountings are available. Standard cabinet finish is Duranodic Bronze; custom paint finishes are available. Sign can be controlled by a switch, Signal-Tech Sign Control Software or third-party relay. Control switch and software can be purchased separately. UL/cUL Listed for wet locations.

**Technical Specifications**

|  |  |
| --- | --- |
| **Illumination** | Backlit with LEDs |
| **LED Message Colors** | Red, Amber, Green, Blue and White |
| **Message** | Standard Font: Swiss 721 Bold BT  Custom font styles, monochrome symbols and graphics available  Message blanks-out when off. |
| **Electrical** | Input voltage 120-277VAC or low volt 12-24VDC  UL/cUL Listed for wet locations |
| **Cabinet Construction**  Single-faced signs; double-faced signs up to 14”H x 18”W  Double-faced signs larger than 14”H x 18”W | One-piece extruded aluminum frame with an 1/8” thick, dark grey diffused acrylic face panel  Available but requires custom engineering |
| **Cabinet Depth** | Single-faced: 2 ½”  Double-faced up to 14”H x 18”W: 5 ½”  Double-faced over 14”H x 18”W: 7 ½” |
| **Cabinet Finish** | Standard: Duranodic Bronze  Options: Custom paint colors or color match paint |
| **IP/NEMA Rating** | IP55/NEMA 3RX |
| **Control** | Switch, Signal-Tech Sign Control Software or external relay |
| **Accessories/Options** | Flashing, Audible Alarm |
| **Warranty** | 2 Years |
| **Country of Origin** | USA |
| **Mounting** | Lift’N Shift sign back offers built in wall mounting (single faced signs only)  Additional mounting can purchased separately: Ceiling, post, recessed |

|  |
| --- |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |