**SBLF Series Indoor LED Backlit Signs**

The SBLF Series Indoor LED Backlit Sign features a block-style message that is readable without illumination. The message is viewable when off and can be illuminated to add emphasis to the message or to optimize readability in low light conditions.

It is engineered with a solid-state circuit board and switch-mode power supply for maximum LED life. The cabinet is constructed of corrosion-resistant, extruded aluminum and ships with our built-in Lift'N Shift back for wall mounting. Ceiling, post, wall-projection and recessed mountings are available. Standard cabinet finish is Duranodic Bronze; custom paint finishes are available. Sign can be controlled by a switch, Signal-Tech Sign Control Software or third-party relay. Control switch and software can be purchased separately. UL/cUL Listed for wet locations.

**Technical Specifications**

|  |  |
| --- | --- |
| **Illumination** | Backlit with white LEDs |
| **Message** | Translucent face color, Font: Swiss 721 Bold BT  Custom font styles, full color symbols and graphics available.  Message always visible; can be illuminated to enhance readability |
| **Electrical** | Input voltage 120-277VAC or low volt 12-24VDC  UL/cUL Listed for wet locations |
| **Cabinet Construction**  Single-faced signs; double-faced signs up to 14”H x 18”W  Double-faced signs larger than 14”H x 18”W | One-piece extruded aluminum frame with an 1/8” thick, clear polycarbonate  Available but requires custom engineering |
| **Cabinet Depth** | Single-faced: 2 ½”  Double-faced up to 14”H x 18”W: 5 ½”  Double-faced over 14”H x 18”W: 7 ½” |
| **Cabinet Finish** | Standard: Duranodic Bronze  Options: Custom paint colors or color match paint |
| **IP/NEMA Rating** | IP55/NEMA 3RX |
| **Control** | Switch, Signal-Tech Sign Control Software or external relay |
| **Accessories/Options** | Audible Alarm, Flashing |
| **Warranty** | 2 Years |
| **Country of Origin** | USA |
| **Mounting** | Lift’N Shift sign back offers built in wall mounting (single faced signs only)  Additional mounting can purchased separately: Ceiling, post, recessed |

|  |
| --- |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |