**Technical Specifications**

**TCL Series Outdoor LED Direct-view Signs**

Indoor/outdoor blank-out signs designed with super bright LEDs and a contrasting face; guaranteed readable in direct sunlight. The sign message is formed by visible LEDs on a black sign face and is designed to illuminate the message or messages when turned on and blank-out or extinguish the message when off. Up to three static messages can be overlaid to reduce the physical footprint of the sign.

It is engineered with a solid-state circuit board and switch-mode power supply for maximum LED life. It has a corrosion resistant, all-weather cabinet and ships with our Lift'N Shift back for wall mounting. Ceiling, post and wall-projection mountings are available. Standard cabinet finish is Duranodic Bronze; custom paint finishes are available. Sign can be controlled by a switch, Signal-Tech Sign Control Software or third-party relay. Control switch and software can be purchased separately. UL/cUL Listed for wet locations. Manufactured in the USA.

|  |  |
| --- | --- |
| Illumination | Super bright, direct-view LEDs |
| LED Message Colors | Red, Amber, Green, Blue and WhiteIndividual LEDs form the message characters |
| Message | Message blanks-out when off.Stock messages or custom messages available |
| Electrical | Input voltage 120-277VAC or low volt 12-24VDCUL/cUL Listed for wet locations |
| **Cabinet Construction** Single-faced signs; double-faced signs up to 14”H x 18”WDouble-faced signs larger than 14”H x 18”W | One-piece extruded, all-weather frame with an 1/8” thick, dark grey diffused acrylic face panelCorrosion resistant, extruded, all-weather frame with two hinged faces. 7.5” deep, mitered construction. Moisture absorbent interior coating1/8” thick smoked-tinted, polycarbonate face panel |
| Cabinet Depth | Single-faced: 2 ½” Double-faced up to 14”H x 18”W: 5 ½”Double-faced over 14”H x 18”W: 7 ½” |
| Cabinet Finish | Standard: Duranodic BronzeOptions: Custom paint colors or color match paint |
| Temperature and Humidity Ratings | The Cabinet and sign components shall operate in the following temperature and humidity conditions: * Operational & storage temperature range: -40°F to +165°F
* Humidity range: 0% to 99% (non-condensing)
 |
| IP/NEMA Rating | IP55/NEMA 3RX |
| Control | Switch, Signal-Tech Sign Control Software or external relay |
| Accessories/Options | Audible Alarm, Flashing, Hoods, Automatic Brightness Dimming |
| Warranty | 5 Years |
| Country of Origin | Manufactured and assembled in the USA |
| Mounting | Lift’N Shift sign back offers built in wall mounting (single faced signs only)Additional mounting can purchased separately: Ceiling, post, side & recessed |